 **ISO/IEC JTC 1/SC 29/ WG 11 N19484**

**ISO/IEC JTC 1/SC 29/WG 11**

**Coding of moving pictures and audio**

**Convenorship: Japan (JISC)**

|  |  |
| --- | --- |
| **Document type:** | Approved WG 11 document |
| **Title:** | Common Test Conditions for MPEG Immersive Video |
| **Status:** | Approved |
| **Date of document:** | 2020-07-25 |
| **Source:** | Convenor, ISO/IEC JTC 1/SC 29/WG 11 |
| **No. of Pages:** | 22 |
| **Email of acting convenor** | [ostermann@tnt.uni-hannover.de](mailto:ostermann@tnt.uni-hannover.de) |
| **Committee URL:** | <http://isotc.iso.org/livelink/livelink/open/jtc1sc29> |
|  |  |

**INTERNATIONAL ORGANISATION FOR STANDARDISATION**

**ORGANISATION INTERNATIONALE DE NORMALISATION**

**ISO/IEC JTC 1/SC 29/WG 11**

**CODING OF MOVING PICTURES AND AUDIO**

**ISO/IEC JTC 1/SC 29/WG 11 N19484**

**Online – July 2020**

|  |  |
| --- | --- |
| **Source:** | **Video** |
| **Title:** | **Common Test Conditions for MPEG Immersive Video** |
| **Editors:** | Joel Jung, Bart Kroon |

**Common Test Conditions for MPEG Immersive Video**

1. **Introduction**

Common test conditions are desirable to conduct coding experiments in a well-defined environment and ease the comparison of the outcome of experiments. This document specifies the common test conditions for ISO/IEC 23090-12 *MPEG Immersive Video* (MIV) related activities. The common test conditions are defined to evaluate the coding efficiency, subjective quality, pixel rate and user experience of immersive video solutions. The technical approach is following these steps:

1. Compress test content,
2. Synthesize intermediate views from decoded views and metadata (when available),
3. Render viewports of real/virtual pose traces with a limited or a wider movement,
4. Evaluate coding efficiency and parallax effect, considering both decoded views and synthesized views.

The bitstream shall be viewer independent, meaning that neither the position nor the orientation of the viewer shall be considered when compressing the test content. The range of supported possible viewer positions is constrained and known.

Two anchors are used that are both based on *Test Model 6 for Immersive Video* (TMIV) [N19483] in combination with HEVC Test Model (HM). the first one, the *MIV anchor*, is a sequence-independent configuration of TMIV + HM, encoding some source views completely while taking only patches of others. The second one, the *MIV view anchor*, is a sequence-independent configuration of TMIV + HM, restricted to encode an automatically determined subset of source views completely, not subdividing views into patches.

1. **Test material**

This section lists the test material that is used by the common test conditions. In Annex A, a detailed description of the sequences is are given, as well as references to input documents, and download links for sequence data and metadata.

CTC-specific configuration files are provided as attachments to this document, as reported in Table 6. The test material is organized in two categories:

* Class CG: computer-generated content, containing CG1 and CG2 sub-categories,
* Class NC: natural content with estimated depth, containing NC1, NC2 and NC3 sub-categories.

The sequences have a common format as defined in the *Call for MPEG-I Visual Test Materials on 6DoF* [N17462] determining texture and depth representations, filenames and metadata. The views are numbered according to the ordering of the metadata files, counting from zero.

The view numbering exists sometimes in a matrix version for the rig description and an ordinal version for the JSON file. Annex 3 “Source View label conversion” gives the correspondence between the two.

The test material is provided as a set of raw sequences, one per view and component (texture or depth). Texture and depth maps sequences characteristics are reported in the following sub-sections. The CG1 and NC1 sequences are named as follows:

v0\_texture\_4096x2048\_yuv420p10le.yuv

v0\_depth\_4096x2048\_yuv420p16le.yuv

using view 0 of ClassroomVideo as an example. The general format is:

**v**ViewNumber**\_**Component**\_**Width**x**Height**\_**VideoFormat**.yuv**

The attachment [A2] includes the json camera parameters to be used for all sequences. The attachment [A4] contains md5sums of the source material.

Table 1 provides a list of mandatory and optional sequences. Optional sequences are challenging content, deliberately difficult to handle. They are not meant for evaluation or promotion of the TMIV.

*Table 1: Mandatory and optional sequences*

|  |  |  |
| --- | --- | --- |
| Mandatory sequences | CG1 – A | ClassroomVideo |
| CG1 – B | Museum |
| CG1 – C | Hijack |
| CG2 – J | Kitchen |
| NC1 – D | Painter |
| NC1 – E | Frog |
| NC1 - P | Carpark |
| CG1 – N | Chess |
| Optional sequences | NC2 – L | Fencing |
| NC1 - U | Street |
| NC1 - T | Hall |
| CG2 - R | Group |
| CG2 - O | Fan |
| CG1 - Q | ChessPieces |

1. **Software tools**

The referenced tools are listed in Table 2, with source code location, documentation and version number.

*Table 2: List of used tools*

|  |  |  |  |
| --- | --- | --- | --- |
| Tool name |  | Location | Tag/branch |
| TMIV | [N19483] | <https://gitlab.com/mpeg-i-visual/tmiv> | v6.0 |
| WS-PSNR | [N18069] | <https://gitlab.com/mpeg-i-visual/wspsnr> | v2.0.1 |
| HM |  | <https://vcgit.hhi.fraunhofer.de/jct-vc/HM.git> | HM-16.16 |
| VMAF | [VMAF] | <https://github.com/Netflix/vmaf> | v1.3.14 |
| IV-PSNR | [N18709] | <https://gitlab.com/mpeg-i-visual/ivpsnr> | V2.0 |

* 1. ***HM***

HEVC Test Model (HM) is used for the MIV anchor and MIV view anchor.

* 1. ***WS-PSNR***

WS-PSNR is a tool in used for computing WS-PSNR or PSNR for objective metrics on images and is used to compare coding and synthesis results against uncompressed source views. For the omnidirectional ERP sequences, computation is done according to §4.2 of [N17197] and is applied to Y, U and V components, but only the Y component is used for evaluation.

The second version of WS-PSNR adds support for perspective images and configuration files using the regular PSNR method.

* 1. ***VMAF***

Video Multimethod Assessment Fusion (VMAF) is an objective full-reference video quality metric. The v0.6.1 4K model that is included with this version of VMAF shall be used.

* 1. ***IV-PSNR***

The PSNR for Immersive Video (IV-PSNR) metric is a full-reference metric based on the PSNR. It includes two major changes: the pixel shift, that considers that edges of the objects in the synthesized view may be shifted due to rounding errors, and the global color shift, that considers that different input views may have various color characteristics.

1. **Anchor definition**

Two anchors are considered to encode the multi-view sequences:

* **MIV anchor**: coding with TMIV + HM, packing some source views completely while taking only patches of others,
* **MIV view anchor**: coding with TMIV + HM, packing a subset of source views completely, not subdividing views into patches.

An algorithmic description of TMIV is provided in [N19483]. HM is configured to encode each video sub bitstream using HEVC Main 10 Level 5.2 random access profile. All configuration parameters for each of the anchors is provided by this document and its attachments.

* 1. ***Coding of the anchor views***

To reduce the burden of anchor generation, without dropping any anchor, it has been decided at 128th MPEG meeting to create a configuration “17fr” with 17 frames only. This configuration is used to compare the anchors against each other. The configuration “97fr”, with 97 frames is mandatory when proposing an improvement of the MIV anchor and is used (optionally) when proposing an improvement of the MIV view anchor. The frame ranges to encode for each sequence are reflected in Table 3, for both “17fr” and “97fr” configurations. Specific details for each anchor are given in the following sub-sections. The attached configuration files [A5], as listed in annex 1, can be used as templates. There are no sequence-dependent codec parameters.

*Table 3:* *Start frames for each configuration.*

|  |  |  |  |
| --- | --- | --- | --- |
| Id | Sequence | “17fr” config. | “97fr” config. |
| CG1 - A | ClassroomVideo | 23 | 23 |
| CG1 - B | Museum | 100 | 100 |
| CG1 - C | Hijack | 0 | 0 |
| CG1 - N | Chess | 60 | 60 |
| CG2 - J | Kitchen | 0 | 0 |
| NC1 - D | Painter | 40 | 40 |
| NC1 - E | Frog | 135 | 135 |
| NC2 - L | Fencing | 30 | 30 |
| NC1 - P | Carpark | 130 | 115 |
| NC1 - U | Street | 225 | 145 |
| NC1 - T | Hall | 80 | 0 |
| CG2 - R | Group | 0 | 0 |
| CG2 - O | Fan | 0 | 0 |
| CG1 - Q | ChessPieces | 60 | 60 |

* 1. ***Coding for MIV anchor***

The coding of the MIV anchor is explained in [N19483]. For each video sequence, two sets of QP points are considered, medium and low, corresponding respectively to QP1, QP2, QP3, QP4, and QP2, QP3, QP4, QP5. The set of QPs for the texture is sequence dependent, to target the 5 to 50 Mbps bitrate range, as defined in Table 4. To each texture QP corresponds one single geometry QP (same mapping for all sequences). The mapping from texture QP (*q*) to geometry QP (*q’*) is given by:

(1)

whereby indicates the rounding to nearest integer operation.

The anchor encodes all source views with geometry input bit depth as reported in tables of Annex A (16 bits for all sequences except Kitchen). The anchor bitstreams themselves include decoded picture hashes for automatic consistency checking.

*Table 4: MIV anchor QPs used to encode texture attribute video sub bitstreams*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sequence Id** | **QP1** | **QP2** | **QP3** | **QP4** | **QP5** |
| **Target bitrate[Mbps]** | **50** | **28** | **16** | **9** | **5** |
| CG1 - A | 25 | 27 | 30 | 33 | 38 |
| CG1 - B | 21 | 27 | 33 | 37 | 41 |
| CG1 - C | 16 | 22 | 29 | 38 | 49 |
| CG2 - J | 14 | 21 | 27 | 33 | 39 |
| CG1 - N | 11 | 18 | 25 | 31 | 38 |
| NC1 - D | 22 | 28 | 35 | 44 | 51 |
| NC1 - E | 30 | 36 | 43 | 47 | 51 |
| NC1 - P | 22 | 26 | 32 | 39 | 47 |
| NC2 - L | 22 | 25 | 32 | 41 | 51 |
| NC1 - T | 15 | 23 | 31 | 40 | 47 |
| NC1 - U | 20 | 24 | 29 | 34 | 41 |
| CG2 - O | 30 | 38 | 45 | 48 | 51 |
| CG2 - R | 24 | 30 | 35 | 40 | 46 |
| CG1 - Q | 4 | 11 | 18 | 26 | 35 |

* 1. ***Coding for MIV view anchor***

The coding of the MIV view anchor is like the MIV anchor. All parameters are the same except for the following:

* maxBasicViewFraction = 1.0
* outputAdditionalViews = false

The texture QPs are defined in Table 5 and the geometry QPs follow from equation (1).

* 1. ***Synthesis of intermediate views***

Both for objective and subjective testing, a range of frames of each sequence are synthesized at source positions. For the synthesis, all decoded atlases are used as input of the view synthesis algorithm. For the objective evaluation, the frames as reported in Table 3 are used for view synthesis.

Proposals are not required to code views corresponding to all anchor-coded views but are required to be able to reconstruct source views and generate viewports for any intermediate view position in the designated range for each test sequence. Each sequence definition includes a virtual view named “viewport” that defines the field of view and resolution of the viewports.

The format of each synthesized view is an omnidirectional image with equirectangular projection with the same angular resolution (pixels / degree) for ERP or semi-ERP test materials, and a linear perspective projection for linear perspective input content. The synthesis result is 10-bit YUV 4:2:0 format for subjective and objective evaluation. Inpainting of invalid pixels is used for both subjective and objective testing.

*Table 5: MIV view anchor QPs used to encode texture attribute video sub bitstreams*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sequence Id** | **QP1** | **QP2** | **QP3** | **QP4** | **QP5** |
| **Target bitrate [Mbps]** | **50** | **28** | **16** | **9** | **5** |
| CG1 - A | 26 | 28 | 30 | 33 | 37 |
| CG1 - B | 24 | 30 | 35 | 38 | 42 |
| CG1 - C | 14 | 18 | 23 | 29 | 35 |
| CG2 - J | 18 | 24 | 29 | 34 | 39 |
| CG1 - N | 10 | 17 | 22 | 28 | 33 |
| NC1 - D | 22 | 28 | 34 | 41 | 47 |
| NC1 - E | 32 | 37 | 42 | 48 | 51 |
| NC1 - P | 22 | 25 | 31 | 37 | 43 |
| NC2 - L | 22 | 24 | 30 | 37 | 45 |
| NC1 - T | 15 | 22 | 29 | 36 | 44 |
| NC1 - U | 21 | 25 | 29 | 34 | 40 |
| CG2 - O | 31 | 37 | 45 | 48 | 51 |
| CG2 - R | 25 | 30 | 34 | 38 | 42 |
| CG1 - Q | 3 | 9 | 15 | 22 | 28 |

1. **Evaluation of proposals**

Only objective and subjective results on mandatory sequences are required for an adoption of a proposal. Additional results obtained on optional sequences can be provided as additional information.

* 1. ***Subjective quality evaluation***

For subjective viewing, each sequence is also synthesized according to a set of pose traces. A pose trace specifies for each frame the position and orientation of the viewport to synthesize. Each pose trace is stored as a comma-separated table with position (X, Y, Z) and orientation (Yaw, Pitch, Roll) columns and exactly one row per frame of the sequence. The format of each synthesized view is an image with perspective projection with at most 2048 × 2048 pixels resolution, at most 90-degree field of view and 10-bit YUV 4:2:0 color format. The purpose is to mimic natural viewing on a head-mounted display (HMD) while using offline tools and a 2D monitor.

Because of the large difference in visual comfort between a viewer that voluntarily initiates head motion versus a viewer watching the same viewport on a 2D monitor, pose traces will have a small amount of motion. For each sequence there are three pose traces – named *X*p01, *X*p02 and *X*p03 – which are meant to represent a diversity of natural head movement compliant with the overall dimension of the capture rig, as indicated in Table 21. Attachment [A3] contains all pose traces. The TMIV decoder is configured to extend the video to 300 frames by mirroring the 97-frame sequences. ClassroomVideo pose traces have been replaced by pose traces that are 300 frames long. The other pose traces are the same as for the CfP [w18145].

It is meaningful to define the pose traces according to the conditions of capture, and typically to define the related path within the volume of the camera rig. It is convenient to formulate this range as a volume in 3D space, as described per sequence in Section 2.

For adoption of a proposed method, the proponent must:

* be able to show any pose trace of the proposed method, during a viewing session.
* be able to show, during the presentation of the contribution, any pose trace, in a side-by-side mp4 format including the anchor, and make it clear what the bitrate and pixel-rate differences with the anchor are.

The command line to be used to generate the side-by-side pose trace is the following:

*ffmpeg.exe -f rawvideo -pix\_fmt yuv420p10le -s:v {width}x{height} -r {fps} -I {anchor yuv} -f rawvideo -pix\_fmt yuv420p10le -s:v {width}x{height} -r {fps} -i {proposed yuv} -profile:v high -c:v libx264 -qp 10 -filter\_complex“"[0:v][1:v]hstack=inputs=”" {output mp4}*

* 1. ***Objective evaluation***

A “**Synthesized view**” corresponds to a source view that is reconstructed through synthesis (view interpolation) by the anchor using the decoded bitstream. All source views are synthesized for objective evaluation, and it is not considered if the source view is fully, partially or not at all present in the bitstream.

The new methods should be compared with the anchor coding results, by reporting the metrics using the attached reporting template. This includes a tab per sequence, a summary sheet and an analysis sheet per metric. BD-rates and averages are automatically calculated to ensure consistent reporting.

For all test classes, WS-PSNR, VMAF and IV-PSNR based BD-rate values will be provided for synthesized source views. For perspective views WS-PSNR reduces to regular PSNR. The comparison of proponents with the anchors will be expressed in terms of BD rate computed on low- and medium bitrate rate-distortion curves.

The BD-rates for anchor and proponent are obtained from:

* The average over each source view and specified frames (Table 3) of the metric between the intermediate view synthesized from decoded atlases and the original/non-compressed source views,
* The total bitrate required to encode the views (including depths) for all frames

For VMAF the geometric average is used. For WS-PSNR and IV-PSNR the average is computed in mean square error (MSE) space.

The reporting template, provided as attachment, should be used for all contributions. This template will compare a proposal with all anchors. Because TMIV makes use of floating-point operations, it is important to report the compiler and operating system that are used for evaluation. Preferred compilers are GCC 7 or newer and VC15. The TMIV software includes a manual with build instructions.

The texture QPs defined for the anchor in section 4.1.1 are defined per sequence, to reach a specific bitrate range. When the proposed method implies bitrate changes compared to the anchor, it might happen that the computed BD-rate returns a zero value (printed as “---”), due to insufficient overlap of the two bitrate vs. metric curves. When this situation occurs for a specific sequence, the proponents should:

* Generate, for the proposal and this sequence specifically, a new point corresponding to a QP0 or QP6 to fall back in the desired bitrate range and allow the BD-rate computation to provide a realistic result. QP0 and QP6 are defined as:

(2)

(3)

* Report in the template the results corresponding to the 5 consecutive QPs that have the largest overlap with the target bitrate range (for instance, QP0, QP1, QP2, QP3, QP4).

When the BD-rate computation still returns a zero value, with the process described above, no average over all sequences will be calculated for this metric. (Instead “---” is printed.) The reporting template includes rate-distortion curves for each metric to study and report the reason for the lack of overlap.

* 1. ***Pixel rate evaluation***

Objective evaluation criteria include pixel rate, which is included in the reporting template. Contributions are required to provide pixel rate for each tested sequence. Proponents should report results which they believe are the most optimal compromise between pixel rate and quality. To provide a meaningful reference for pixel rate values, the following constraints are defined:

**Low pixel rate test condition constraints:**

* The combined maximum luma sample rate across all decoders is maximally 1,069,547,520 samples per second (e.g. 32 MP @ 30 fps, corresponding to HEVC Main 10 profile @ Level 5.2)
* Each decoder instantiation is constrained to a maximum luma picture size of 8,912,896 pixels (e.g. 4096 x 2048, corresponding to HEVC Main 10 profile @ Level 5.2).
* The maximum number of simultaneous decoder instantiations is four.

**High pixel rate test condition constraints:**

* The combined maximum luma sample rate across all decoders is maximally 4,278,190,080 samples per second (e.g. 128 MP @ 30 fps, corresponding to HEVC Main 10 profile @ Level 6.2)
* Each decoder instantiation is constrained to a maximum luma picture size of 35,651,584 pixels (e.g. 8192 x 4096, corresponding to HEVC Main 10 profile @ Level 6.2).
* The maximum number of simultaneous decoder instantiations is four.

These conditions are orthogonal to low/high bitrate conditions. The MIV anchor and the MIV view anchor satisfy the low pixel rate test condition constraints. In fact, the test model automatically determines suitable atlas frame sizes based on these constraints.

There is currently no test sequence or anchor that targets the high pixel rate test condition constraints.

* 1. ***Runtimes evaluation***

Runtimes should be reported for anchors and proposals (corresponding cells in the reporting template are mentioned):

* Atlas generation (incl. all preprocessing), cells M267 to M271 and AA267 to AA271.
* HM encoding of texture and depth atlases, cells M4 to M128 and AA4 to AA128, M140 to M264 and AA140 to AA264.
* HM decoding of texture and depth atlases, cells N4 to N128 and AB4 to AB128, N140 to N264 and AB140 to AB264.
* Rendering (incl. all postprocessing), cells N285 to N409 and AB285 to AB409.

The reference software includes measurement of CPU runtime, excluding loading from disk and writing to disk. Proposals should include a similar runtime measurement.

It is reminded that the proponent has to fill the runtimes for both anchor and proposed method, so that the delta between anchor and proposal runtimes has a meaning.

1. **References**

[VMAF] [vmaf: Perceptual video quality assessment based on multi-method fusion](https://github.com/Netflix/vmaf), Netflix, Inc., 2017-07-14.

[N18068] Reference View Synthesizer (RVS) manual, ISO/IEC JTC1/SC29/WG11 MPEG/N18068, October 2018, Macau SAR, China.

[N18069] ERP WS-PSNR manual, ISO/IEC JTC1/SC29/WG11 MPEG/N18069, October 2018, Macau SAR, China.

[N17197] Algorithm descriptions of projection format conversion and video quality metrics in 360Lib Version 5, JVET-H1004, ISO/IEC JTC1/SC29/WG11 MPEG/N17197, October 2017, Macau SAR, China.

[N18145] Call for Proposals on 3DoF+ Visual, ISO/IEC JTC1/SC29/WG11 MPEG/N18145, January 2019, Marrakesh, Morocco.

[N19483] Test Model 6 for Immersive Video, ISO/IEC JTC1/SC29/WG11 MPEG/N19483, July 2020, Online.

[N18709] Software manual of IV-PSNR for Immersive Video, ISO/IEC JTC1/SC29/WG11 MPEG/N18709, July 2019, Gothenburg, Sweden.

1. **List of attachments**

Table 6 provides an overview of files that are provided together with this document. Attachments [A1], [A2], [A3] and [A4] are also included as part of the TMIV reference software.

Table 6: List of attachments to this document

|  |  |  |
| --- | --- | --- |
| **ID** | **Filename** | **Short description** |
| [A1] | template.zip | Excel reporting template |
| [A2] | tmiv\_camparam.zip | Metadata files according to the updated format [w18068] with source and intermediate view positions for all sequences (omnidirectional and perspective) |
| [A3] | tmiv\_posetraces.zip | Three pose traces per sequence |
| [A4] | source\_md5.zip | MD5 sums for all source data |
| [A5] | tmiv\_configs.zip | Template configuration files for SA |

**Annex A: test sequences characteristics**


***Computer-generated content***

**ClassroomVideo**

The general characteristics of the ClassroomVideo sequence are summarized in Table 7. Source view positions are according to a hexagonally-packed circular disc with an additional top and bottom view, as shown in Figure 1.

*Table 7: Characteristics of the ClassroomVideo sequence*

|  |  |
| --- | --- |
| Category – Short name | CG1 – SA |
| Input contributions | m42415, m42756 and m42944 |
| Length & frame rate | 120 frames (30 fps) |
| Number of source views | 15 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits, normalized disparity in [0.8m, ) range |
| Source view resolution | 4096 × 2048 |
| View FoV & mapping | 360° × 180° ERP |
| Global FoV | 360° × 180° |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent /MPEG-I/Philips/ClassroomVideo/CE/  Data: v\*.zip |



*Figure 1: Visualization of the view positions of the ClassroomVideo sequence*


The viewing space volume is a spheroid centered at source view v0 eg (0, 0, 0) meter position, with equatorial radius 104 mm and polar distance 60 mm:

**Museum**

The general characteristics of the Museum sequence are summarized in Table 8. The cameras are disposed on a spherical surface of 30 cm radius, and divergent in the direction of the sphere radius. Figure 2 provides the (X, Y, Z) coordinates and the spherical dimension, with an example using the 11th view. The metadata file comprising source and intermediate view positions is attachment A12 to this output document.

*Table 8: Characteristics of the Museum sequence*

|  |  |
| --- | --- |
| Category – Short name | CG1 - SB |
| Input contribution | m42349 |
| Length & frame rate | 300 frames (30 fps) |
| Number of source views | 24 |
| Source view resolution | 2048 × 2048 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits, normalized disparity in [0.5m, 25m] range |
| View FoV & mapping | 180° × 180° ERP |
| Global FoV | 360° × 180° |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/ MPEG-I/Technicolor/TechnicolorMuseum/CE/  Data: TechnicolorMuseumV\*.zip |



*Figure 2: Coordinate system as used by 3D Audio and OMAF, with view 10 of the Museum sequence superimposed*


The viewing space volume is a sphere centered at position [0, 0, 1.65] meter with a 300 mm radius:

**Hijack**

The general characteristics of the Hijack sequence are summarized in Table 9. Figure 3 provides a visualization of the virtual camera rig in bias, top and front view respectively. The metadata file comprising source and intermediate view positions is in attachment [A2] of this output document.

*Table 9: Characteristics of the Hijack sequence*

|  |  |
| --- | --- |
| Category – Short name | CG1 - SC |
| Input contribution | m42349 |
| Length & frame rate | 300 frames (30 fps) |
| Number of source views | 10 |
| Source view resolution | 4096 × 2048 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits, normalized disparity in [0.5m, 25m] range |
| View FoV & mapping | 180° × 90° ERP |
| Global FoV | 180° × 90° |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent /MPEG-I/Interdigital/InterdigitalHijack/  Data: vAll\_depth\_4096x2048\_yuv420p16le.zip  vAll\_texture\_4096x2048\_yuv420p10le.zip |



*Figure 3: Visualization of the view positions of the Hijack sequence*

The viewing space volume is a sphere centered at position [0, 0, 1.65] meter with a 300 mm radius:

**Group**

The general characteristics of the Group sequence are summarized in Table 10 and source view positions illustrated in Figure 4.




Figure 4: Visualization of the view positions of the Group sequence

The captured views form a partial dome of 21 views made of lower, middle and upper arc shape row, roughly span over 180° and looking inward to a central scene.

*Table 10: Characteristics of the Group sequence*

|  |  |
| --- | --- |
| Category - Name | CG2 - R |
| Input contribution | m54731 |
| Length & frame rate | 99 frames (30 fps) |
| Number of source views | 21 |
| Source view resolution | 1920x1080 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 75° × 48° Rectilinear |
| Camera spacing | 12 cameras span on #180° of arc radius 4.0m, height 2.5 m tilt 25°  6 cameras span on #180° of arc radius 2.75m, height 4.0 m tilt 45°  3 cameras span on #180° of arc radius 2.0m, height 5.0 m tilt 60° |
| zNear | 1.5 m |
| zFar | 25.0 m |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Interdigital/Interdigital\_Group\_Content  Data: v\*.zip |

The viewing space volume is a flat volume which would be wrapped around this partial half dome.

**Fan**

The general characteristics of the Fan sequence are summarized in Table 11. The rig is a planar rectangular rig of 5 by 3 cameras with a slight tilt downward.

*Table 11: Characteristics of the Fan sequence*

|  |  |
| --- | --- |
| Category - Name | CG2 - O |
| Input contribution | m54732 |
| Length & frame rate | 97 frames (30 fps) |
| Number of source views | 15 |
| Source view resolution | 1920x1080 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 50° horizontal Rectilinear |
| Camera spacing | 5 x 3 rectangular rig spaced by 10cm horizontally and vertically  1st row: v0 to v4  2nd row: v5 to v9  3rd row: v10 to v14 |
| zNear | 0.35 m |
| zFar | 12.5 m |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Interdigital/Interdigital\_Fan\_Content  Data: v\*.zip |

The viewing space volume is a spheroid encompassing the 15 cameras.

**ChessPieces**

The general characteristics of the ChessPieces sequence are exactly the same as Chess and summarized in Table 12. The notable differences between Chess and ChessPieces are:

* ChessPieces has an improved utilization of depth range, which is now adjusted per source view to the actual minimum and maximum,
* Additional inclusion of entity maps which annotate physical objects and is provided each input source view. The sequence contains roughly 60 separate indexed entities.

*Table 12: Characteristics of the ChessPieces sequence*



|  |  |
| --- | --- |
| Category - Name | CG1 - Q |
| Input contributions | m54382 |
| Length & frame rate | 300 frames (30 fps) |
| Number of source views | 10 |
| Texture format | YUV 4:2:0 10-bits |
| Depth format | YUV 4:2:0 16-bits, normalized disparity in (0.1m,m) sub range |
| Source view resolution | 2048 × 2048 |
| View FoV & mapping | 180° × 180° ERP |
| Global FoV | 360° × 180° |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Nokia/MIV/NokiaChessNew  Data: v\*.tgz |

**Chess**

The general characteristics of the Chess sequence are summarized in Table 13. In total there are ten source cameras, laid out in a sphere-like arrangement as illustrated in Figure 5. One camera in the constellation captures the top of the scene and another the bottom. The remaining eight cameras are pointing outwards to capture the rest of the scene. The radius of the spherical camera constellation is 30 cm. This sequence also comes with a ground truth pose-trace viewport video.

*Table 13: Characteristics of the Chess sequence*

|  |  |
| --- | --- |
| Category – Short name | CG1 - SN |
| Input contributions | m50787 |
| Length & frame rate | 300 frames (30 fps) |
| Number of source views | 10 |
| Texture format | YUV 4:2:0 10-bits |
| Depth format | YUV 4:2:0 16-bits, normalized disparity in (0.1m,m) range |
| Source view resolution | 2048 × 2048 |
| View FoV & mapping | 180° × 180° ERP |
| Global FoV | 360° × 180° |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Nokia/MIV/NokiaChess  Data: v\*.tgz |



*Figure 5: visualization of the camera constellation for Chess*

The viewing space volume is a sphere centered at position [-0.5, -0.5, 1.0] meter with a 300 mm radius:

**Kitchen**

The general characteristics of the Kitchen sequence are summarized in Table 14 and source view positions in Table 23. The captured views form a 5 × 5 planar array and are numbered v0-0 to v4-4 following left to right and top to bottom scan order.

*Table 14: Characteristics of the Kitchen sequence*

|  |  |
| --- | --- |
| Category – Short name | CG1 - SJ |
| Input contribution | m43318 |
| Length & frame rate | 97 frames (30 fps) |
| Number of source views | 25 (5x5) |
| Source view resolution | 1920x1080 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 10 bits |
| View FoV & mapping | 53.1° × 31.4° Rectilinear |
| Lens | 32 mm |
| Camera spacing | 20cm x 20cm |
| zNear | 2.2 |
| zFar | 7.2 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Orange/OrangeKitchen/CE  Data: v\*.zip |

The viewing space volume is a spheroid centered at position [0, -0.4, 0.4] meter, covering a vertical square of side equal to 0.8m and developed in the forward axis by 0.35m max.

***Natural content with estimated depth***

**Painter**

The general characteristics of the Painter sequence are summarized in Table 15 and source view naming in Table 22 form a 4x4 planar array and are numbered v0-0 to v3-3 following left to right and top to bottom scan order, as shown in Table 16. The refined depths proposed in [m47445] are used.

*Table 15: Summary of the Painter sequence*

|  |  |
| --- | --- |
| Category – Short name | NC1 - SD |
| Input contributions | m40010, m40011, m43366 and m47445. |
| Length & frame rate | 300 frames (30 fps) |
| Number of source views | 16 (4x4) |
| Source view resolution | 2048 × 1088 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Technicolor/TechnicolorPainter/CE/  Data: TechnicolorPainterV\*.zip |

*Table 16: View numbering of the Painter camera array*

|  |  |  |  |
| --- | --- | --- | --- |
| v0-0 | v1-0 | v2-0 | v3-0 |
| v0-1 | v1-1 | v2-1 | v3-1 |
| v0-2 | v1-2 | v2-2 | v3-2 |
| v0-3 | v1-3 | v2-3 | v3-3 |

The viewing space volume is a spheroid centered at position [0, -0.35, -0.35] meter, covering a vertical square of side equal to 20cm and developed in the forward axis by 25cm max.

**Frog**

The general characteristics of the Frog sequence are summarized in Table 17 and source view positions in Table 24. The captured views form a 15x1 line and are numbered v0-0 to v14-0 following left to right scan order. The refined depths proposed in [m47445] are used; these depths do not exist for extreme view positions v0 and v14 and therefore only the views from v1 to v13 are used.

*Table 17: Characteristics of the Frog sequence*

|  |  |
| --- | --- |
| Category – Short name | NC1 - SE |
| Input contribution | m43748, m44914 and m47445 |
| Length & frame rate | 300 frames (30fps) |
| Number of source views | 13 (13x1) |
| Source view resolution | 1920x1080 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 63.65° × 38.47° Rectilinear |
| Lens | 2.16 mm |
| Camera spacing | 3.675 cm |
| zNear | 0.3 |
| zFar | 1.62 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Intel/Frog/CE  Data: IntelFrog\_\*.zip |

The viewing space volume is a rectangle centered at position [0, 0, 0] meter with a 15cm width, 44.1cm length, and no z component.

**Fencing**

The general characteristics of the Fencing sequence are summarized in *Table 18* and source view positions in Table 25. The captured views form a 10x1 linear arc and are numbered v0-0 to v9-0 following left to right scan order.

*Table 18: Characteristics of the Fencing sequence*

|  |  |
| --- | --- |
| Category – Short name | NC1 - SL |
| Input contribution | m38247 |
| Length & frame rate | 250 frames (25 fps) |
| Number of source views | 10 |
| Source view resolution | 1920x1080 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 63° × 48° |
| Lens | 4.5 mm |
| Camera spacing | 5 stereopairs (baseline: 22 cm) placed on arc (radius: 4 m),  angle between neighboring stereopairs: 15 degrees,  total angle of the system: 60 degrees |
| zNear | 3.5 |
| zFar | 7.0 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Poznan/Poznan\_Fencing2/CE  Data: PoznanFencing\_\*.zip |

**Street**

The general characteristics of the Street sequence are summarized in Table 19. The captured views form a 9x1 line and are numbered v0 to v8 following left to right scan order.

*Table 19: Characteristics of the Street sequence*

|  |  |
| --- | --- |
| Category – Short name | NC1 – SU |
| Input contribution | m51598 |
| Length & frame rate | 250 frames (25fps) |
| Number of source views | 9 (9x1) |
| Source view resolution | 1920x1088 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 63° × 48° |
| Lens | 4.5 mm |
| Camera spacing | 13.75 cm |
| zNear | 34.5064 |
| zFar | 2760.511 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Poznan/PoznanStreet  Data: PoznanStreet\_\*.zip |

**Carpark**

The general characteristics of the Carpark sequence are summarized in Table 20. The captured views form a 9x1 line and are numbered v0 to v8 following left to right scan order.

*Table 20: Characteristics of the Carpark sequence*

|  |  |
| --- | --- |
| Category – Short name | NC1 – SP |
| Input contribution | m51598 |
| Length & frame rate | 250 frames (25fps) |
| Number of source views | 9 (9x1) |
| Source view resolution | 1920x1088 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 63° × 48° |
| Lens | 4.5 mm |
| Camera spacing | 13.75 cm |
| zNear | 34.5064 |
| zFar | 2760.511 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Poznan/PoznanCarpark  Data: PoznanCarpark\_\*.zip |

**Hall**

The general characteristics of the Hall sequence are summarized in Table 21. The captured views form a 9x1 line and are numbered v0 to v8 following left to right scan order. Camera rig in the Hall sequence was moving along the scene, but camera parameters remained the same for all frames.

*Table 21: Characteristics of the Hall sequence*

|  |  |
| --- | --- |
| Category - Name | NC1 – T |
| Input contribution | m51598 |
| Length & frame rate | 500 frames (25fps) |
| Number of source views | 9 (9x1) |
| Source view resolution | 1920x1088 |
| Texture format | YUV 4:2:0 10 bits |
| Depth format | YUV 4:2:0 16 bits |
| View FoV & mapping | 63° × 48° |
| Lens | 4.5 mm |
| Camera spacing | 13.75 cm |
| zNear | 18.5064 |
| zFar | 2760.511 |
| Download | http://mpegfs.int-evry.fr/mpegcontent/ws-mpegcontent/MPEG-I/Poznan/PoznanHall  Data: PoznanHall\_\*.zip |

The viewing space volume is an arc centered at the origin with a 2.34m width, 6.89m length, and no z component.

**Annex B: Source view label conversion**

*Table 22: View naming of the Painter sequence*

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Original view name | Json view name | Original view name | Json view name | Original view name | Json view name | Original view name | Json view name |
| v0-0 | v0 | v1-0 | v1 | v2-0 | v2 | v3-0 | v3 |
| v0-1 | v4 | v1-1 | v5 | v2-1 | v6 | v3-1 | v7 |
| v0-2 | v8 | v1-2 | v9 | v2-2 | v10 | v3-2 | v11 |
| v0-3 | v12 | v1-3 | v13 | v2-3 | v14 | v3-3 | v15 |

*Table 23: View naming of the Kitchen sequence*

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Original view name | Json view name | Original view name | Json view name | Original view name | Json view name | Original view name | Json view name | Original view name | Json view name |
| v0-0 | v00 | v0-1 | v05 | v0-2 | v10 | v0-3 | v15 | v0-4 | v20 |
| v1-0 | v01 | v1-1 | v06 | v1-2 | v11 | v1-3 | v16 | v1-4 | v21 |
| v2-0 | v02 | v2-1 | v07 | v2-2 | v12 | v2-3 | v17 | v2-4 | v22 |
| v3-0 | v03 | v3-1 | v08 | v3-2 | v13 | v3-3 | v18 | v3-4 | v23 |
| v4-0 | v04 | v4-1 | v09 | v4-2 | v14 | v4-3 | v19 | v4-4 | v24 |

*Table 24: View naming of the Frog sequence*

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Original view name | Json view name | Original view name | Json view name | Original view name | Json view name | Original view name | Json view name |
| cam00 | v14 | cam04 | v10 | cam08 | v06 | cam12 | v02 |
| cam01 | v13 | cam05 | v09 | cam09 | v05 | cam13 | v01 |
| cam02 | v12 | cam06 | v08 | cam10 | v04 | cam14 | v00 |
| cam03 | v11 | cam07 | v07 | cam11 | v03 |  |  |

*Table 25: View naming of the Fencing sequence*

|  |  |  |  |
| --- | --- | --- | --- |
| Original view name | Json view name | Original view name | Json view name |
| v0-0 | v00 | v5-0 | v05 |
| v1-0 | v01 | v6-0 | v06 |
| v2-0 | v02 | v7-0 | v07 |
| v3-0 | v03 | v8-0 | v08 |
| v4-0 | v04 | v9-0 | v09 |